Q. Is is possible to connect a HMI tag to the OPC UA server address?

A. No it is not possible. OPC UA server IP address can only be configured from the PLC in the TIA portal.